Requirement of ScalesNet

Customer name:…………………………………………………………………...

City/Country .……………………………………………………………………...

PC for ScalesNet Server…………………………………………………………..

Hardware suitably for Windows 7/8/10 or Windows Server 2003/2008 or higher

Processor Intel i7 and at least 16 GB of RAM

More freely hard disk memory> 20 GB

If laptops are connected via Ethernet or Robots are using with ScalesNet is a Network   
Module reqiuered.

Network modul for ScalesServer ………………………………………………..

Microsoft Word® is required.

Laptop for ScalesNet-ScalesMass………………………………….....................

Hardware suitably for Windows 7/8/10

at least 8 GB RAM

optional WLAN IEEE 802.11/n (>100 MBit/sec recommended)

Optional WLAN Acces Point……………………………………………………

Ready for operation for access of the laptop in the network

Printer……………………………………………………………………………..

Network printer or a local Printer on ScalesServer PC

Comparators  
List all used balances, Comparators, Handler and Robots: e.g. CCE6, AX206 etc.

………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………

For installing of ScalesNet local administration rights on all PC's and laptops

are strictly necessary.

Climate stations (data loggers)

How many climate station are in use? ……….. (the logger can have 1 …n probes)

Which climate stations (data loggers) are used:

Data loggers are connected via RS232 or TCP/IP:

Sartorius ……….……………………..

Technetics microsens ….…………………..

Vaisala ...........................……...…….

Black Stack …......................…………….

Lufft Opus20 .........................………….….

Dostmann P655 Temperature, Humidity..…

Testo Hygrotest 600/650 ..…………….

Other manufacturer .....................………..

Other manufacturer of climate stations:..…………………………………………

……………………..………………………………………………………………

……………………..………………………………………………………………

……………………..………………………………………………………………

Miscellaneous  
 How many associates calibrate weights at the same time?............................

Dissemination required?..................................................................................

On-Site Module required?........………………………………………………

Important

Only TeamViewer is required for remote support and is provided free of charge.

An example of configuratoin:

The lab has 5 manual comparators, 1 load alternator, 1 climate station and calibrate class E2

If two employees calibrate weights on different manual balances, one load alternator runs at the same time and 1 climate station is connected (unlimited probes)

The following licences are required:

1. 1x ScalesNet Basic + Network (consist of 1x ScalesServer, 1x ScalesDesk,   
   2x ScalesMass, 1x ScalesPrinter, 1x Network license)
2. 1x ScalesNet load alternator (consist of 1x ScalesMass)
3. 1x ScalesNet Module OIML class E, ASTM 000,00,0,1

ScalesNet is hardlock protected and the purchased licenses are stored in the hardlock.

In case of loss of the hardlock no replacement will be delivered